
**Practical No. 3**

1. **Using Packet Tracer, create a basic network of One server and two computers using appropriate network wire. Use Dynamic IP address allocation and show connectivity.**


**Step 1: Select ‘End Devices’ and select ‘Server’**




**Step 2: Drag and drop the ‘Server’**



**Step 3: Select ‘Network Devices’, select ‘Switch’ and select ‘PT Switch’**




**Step 4: Drag and drop the ‘PT Switch’**




**Step 5: Select ‘End Devices’ and select ‘PC’ and ‘Laptop’**







**Step 6: Drag and drop 2 ‘PC’s**




**Step 7: Select ‘Connections’ and select ‘Copper Straight Through’**




**Step 8: Connect all devices with fastethernet**




**Step 9: Give start IP name 192.168.0.0**




**Step 10: Select ‘Server’ and go to ‘IP Configuration’**




**Step 11: Go to ‘Desktop’ give ‘Static IP’ and ‘subnet nask’**




**Step 12: Go to ‘Services’ and give default gateaway and DNS**




**Step 13: Click ‘save’**




**Step 14: Select every PC and select DHCP**



**Step 15: Connections Completed**



**Step 16: Assign Packets**



**Step 17: Run Simulation**

